{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":8,"rows_kept":11,"merged":[[1,0,1,7],[10,0,10,7]],"flags":["formulas_cached_only"]}
["附件3："]
["计控室计量水表及附属材料报价单"]
["序号","设备名称","型号/规格/参数","单位","数量","单价（元）","总价（元）","备注"]
[1,"超声波流量计","型号/规格：BLCS-L-F-W                                                                                                                                                                               安装方式：外夹式；                                                                                                                                                              测量介质：生活水；                                                                              管径：DN50-DN300；                                                                             管道材质：钢管、铸铁；                                                                                         常用流量：t/h；                                                                                                         测量精度：1级；                                                                                         防护等级：IP68；                                                                                              一次检测元件工作在水中；                                                                                     电源：220VAC；                                                                                   配置RS232和RS485通讯接口；提供通讯技术协议；与数据采集路由器配套实现远距里计量数据上传、接收、显示；                                                                                                                                                                       带配套安装附件和辅材； ","套",13,null,null,"附带安装、调试"]
[2,"电磁流量计","型号/规格： BLDC-Y-R                                                                                            测量介质：水；\n防护等级：IP68；                                                                                                                                                                                   电源：220VAC； \n配置安装连接附件；\n配置RS232和RS485通讯接口，并提供通讯协议；","个",1,null,null,"附带安装、调试"]
[3,"仪表控制箱","与超声波流量计转换器成套的仪表箱（含电源开关配置、箱内连接线；箱内预留流量计转换器、数据采集路由器安装空间和安装配件）；参考尺寸；宽×高×厚=500×400×200mm；厚：1.0mm;室外安装；防雨防雪防尘；","个",14]
[4,"数据采集路由器（计量模块）","                                                      品牌：Baimatech 佰马科技                                                        规格型号：BMR200-A  \nIndustrial Router\nTDD/FDD\n","台",14]
[5,"电缆","RVV-3×1.5","米",1000]
[6,"信号电缆","ZR-RVVP-2×1.0","米",1000]
[null,"小计"]
["注：所有流量计配套仪表箱，内含电源开关、仪表卡槽及接线端子排。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}