{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["螺旋输送机","斗式提升机","储气罐","高速过滤器","导轨、头部星轮","环冷机台车","齿圈、齿轮","滑板","阀门"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"螺旋输送机","index":0,"n_rows":20,"n_cols":14,"rows_kept":20,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[13,0,13,4],[14,0,14,9],[16,0,16,16],[17,0,17,16],[18,0,18,16],[19,0,19,3],[19,10,19,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":11},"A标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0201018037","螺旋输送机"," GX型（详细型号按照报价单位型号填写）","螺旋直径：φ400； 输送长度：34.5m；输送量：23m3/h 螺旋机制法：S；输送物料：布袋灰；螺旋轴转速：48r/min 螺旋机倾角：0°；驱动装置型号：YTC902-11-48-80","套",1,{"$nulls":5},"订货图SS2032-2-10Q5-3；所有电气设施为防爆、防水、防尘、防静电","炼铁厂8高炉粗煤气系统大修"]
[2,"0201018038","螺旋输送机"," GX型（详细型号按照报价单位型号填写）","螺旋直径：φ400； 输送长度：24.5m；输送量：23m3/h 螺旋机制法：S；输送物料：布袋灰；螺旋轴转速：32r/min 螺旋机倾角：0°；驱动装置型号：YTC902-7.5-32-80","套",1,{"$nulls":5},"详见订货图SS2032-2-10Q5-4更换2#螺旋输送机 设备生产前先与现场尺寸核对无误后再生产；所有电气设施为防爆、防水、防尘、防静电","炼铁厂8高炉粗煤气系统大修"]
[3,"0303025003007","双轴螺旋加湿卸灰机","YJS450","入口2个，接管尺寸φ159*10","套",1,{"$nulls":5},"设备地脚螺栓及外部接口尺寸严格按图SS2032-06Q3-3执行；配套电机，防爆防水防尘防静电","炼铁厂8高炉粗煤气系统大修"]
[4,"0303025004018","仓壁振动器","TZF-6",null,"个",4,{"$nulls":5},"所有电气设施为防爆、防水、防尘、防静电","炼铁厂8高炉粗煤气系统大修"]
[5,"0303025004019","仓壁振动器","TZF-10",null,"个",4,{"$nulls":5},"所有电气设施为防爆、防水、防尘、防静电","炼铁厂8高炉粗煤气系统大修"]
[6,"0303025004020","星形卸灰阀","HFL9B48W-2.5Q   DN300","长度：540mm，轴头密封，带配对法兰及连接件","个",2,{"$nulls":5},"所有电气设施为防爆、防水、防尘、防静电","炼铁厂8高炉粗煤气系统大修"]
[7,"0303020001052","电液动扇形闸门","50B60","500*500，法兰为600*600","台",4,{"$nulls":6},"炼铁厂八高炉矿槽系统改造工程"]
[8,"0303020001051","电液动扇形闸门","50B60","500*500，法兰为600*600","台",2,{"$nulls":6},"炼铁厂八高炉矿槽系统改造工程"]
[9,"0303020001050","反向称门","60x50B45","FFZM-60*50B45-II","台",8,{"$nulls":6},"炼铁厂八高炉矿槽系统改造工程"]
[{"$nulls":6},13]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"斗式提升机","index":1,"n_rows":12,"n_cols":14,"rows_kept":12,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[5,0,5,4],[6,0,6,9],[8,0,8,16],[9,0,9,16],[10,0,10,16],[11,0,11,3],[11,10,11,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":11},"B标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0201018039","斗式提升机","TH315-SH-Y7Y140-16.02","减速机：EQ400，左右各布置1台；电机型号YBX3-132M-4  7.5Kw","台",2,{"$nulls":5},"减速机左、右布置各1台；更换现有斗式提升机，设备生产前先与现场尺寸核对无误后再生产；所有电气设施为防爆、防水、防尘、防静电","炼铁厂8高炉粗煤气系统大修"]
[{"$nulls":6},2]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"储气罐","index":2,"n_rows":12,"n_cols":14,"rows_kept":12,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[5,0,5,4],[6,0,6,9],[8,0,8,16],[9,0,9,16],[10,0,10,16],[11,0,11,3],[11,10,11,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":11},"C标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0201015038","储气罐","详见图：SS2032-2-10Q3-3","介质：氮气 容积：25m3 设计压力：1.6MPa 工作压力≤1.0MPa","台","1",{"$nulls":6},"炼铁厂8高炉粗煤气系统大修"]
[{"$nulls":6},1]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"高速过滤器","index":3,"n_rows":12,"n_cols":14,"rows_kept":12,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[5,0,5,4],[6,0,6,9],[8,0,8,16],[9,0,9,16],[10,0,10,16],[11,0,11,3],[11,10,11,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":11},"D标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0201016026","高速过滤器","处理水量：180t/h  工作压力：0.6MPa","直径φ2400,材质：碳钢，DN200电动蝶阀4台，DN150电动蝶阀1台，DN80电动蝶阀1台，DN200手动蝶阀4台，DN150手动蝶阀1台，DN80手动蝶阀1台，成套PLC控制装置,手动、时间、压差控制1套，N=300W/220V，压力表、压力变送器、自动排气阀1套，带进出口配对法兰及连接件，带填料及布水管路，所有蝶阀带配对法兰及连接件，人孔、顶部钢平台及爬梯1套。","台","1",{"$nulls":6},"炼钢厂"]
[{"$nulls":6},1]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"导轨、头部星轮","index":4,"n_rows":55,"n_cols":14,"rows_kept":55,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[48,0,48,4],[49,0,49,9],[51,0,51,16],[52,0,52,16],[53,0,53,16],[54,0,54,3],[54,10,54,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":12},"E标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0302002003009","右导轨（头4#）","13B379-22-4","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[2,"0302002003001","右导轨（头4#）","13B404-7-7","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[3,"0302002003002","右导轨（头6#）","13B404-7-10","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[4,"0302002003010","右导轨（头6#）","13B379-22-3","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[5,"0302004004003","右导轨（尾13#）","13B379-23-5","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[6,"0302004004004","右导轨（尾17#）","13B379-23-6","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[7,"0302004004001","右导轨（尾3#）","13B379-23-3","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[8,"0302004004005","右导轨（尾45#）","13B379-23-11","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[9,"0302004004006","右导轨（尾47#）","13B379-23-12","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[10,"0302004004007","右导轨（尾49#）","13B379-23-13","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[11,"0302004004002","右导轨（尾6#）","13B379-23-4","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[12,"0302004003001","右左导轨（尾23#/36#）","13B379-23-7","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[13,"0302004003001","右左导轨（尾23#/36#）","13B379-23-7","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[14,"0302004003002","右左导轨（尾29#/30#）","13B379-23-8","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[15,"0302004003002","右左导轨（尾29#/30#）","13B379-23-8","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[16,"0302004003003","右左导轨（尾30#/26#）","13B379-23-9","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[17,"0302004003003","右左导轨（尾30#/26#）","13B379-23-9","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[18,"0302004003004","右左导轨（尾41#/18#）","13B379-23-10","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[19,"0302004003004","右左导轨（尾41#/18#）","13B379-23-10","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[20,"0302004003005","右左导轨（尾55#/6#）","13B379-23-14g","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[21,null,"右左导轨（尾55#/6#）","13B379-24-57g","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[22,"0302002001005","左导轨（头14#）","13B404-6-13","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[23,"0302002001015","左导轨（头14#）","13B379-22-8","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[24,"0302002001011","左导轨（头4#）","13B404-7-20","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[25,"0302002001001","左导轨（头4#）","13B404-6-5","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[26,"0302002001006","左导轨（头41#）","13B404-6-17","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[27,"0302002001014","左导轨（头41#）","13B379-22-9","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[28,"0302002001013","左导轨（头43#）","13B404-7-22","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[29,"0302002001007","左导轨（头43#）","13B404-6-18","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[30,"0302002001012","左导轨（头44#）","13B404-7-21","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[31,"0302002001008","左导轨（头44#）","13B404-6-19","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[32,"0302002001010","左导轨（头6#）","13B404-7-16","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[33,"0302002001002","左导轨（头6#）","13B404-6-8","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[34,"0302002001009","左导轨（头7#）","13B404-7-14","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[35,"0302002001003","左导轨（头7#）","13B404-6-9","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[36,"0302002001016","左导轨（头9#）","13B379-22-7","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[37,"0302002001004","左导轨（头9#）","13B404-6-11","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[38,"0302002002004","左右导轨（头1#）","13B379-22-6","50Mn","件",4,{"$nulls":6},"4号烧结机大修"]
[39,"0302002002001","左右导轨（头1#）","13B379-8-3","50Mn","件",4,{"$nulls":6},"4号烧结机大修"]
[40,"0302002002002","左右导轨（头3#）","13B404-7-6","50Mn","件",2,{"$nulls":6},"4号烧结机大修"]
[41,"0302002002003","左右导轨（头3#）","13B404-7-11","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[42,"0302002002002","左右导轨（头3#）","13B404-7-6","50Mn","件",2,{"$nulls":6},"4号烧结机大修"]
[43,"0302002002005","左右导轨（头3#）","13B379-22-5","50Mn","件",1,{"$nulls":6},"4号烧结机大修"]
[44,"0302003001018","头部星轮装配","13B450-3-2","右传动","套",1,{"$nulls":6},"4号烧结机大修"]
[{"$nulls":6},52]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"环冷机台车","index":5,"n_rows":12,"n_cols":14,"rows_kept":12,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[5,0,5,4],[6,0,6,9],[8,0,8,16],[9,0,9,16],[10,0,10,16],[11,0,11,3],[11,10,11,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":12},"F标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0302012001006","环冷机台车","HL235A.1.2","详见图纸","件",26,{"$nulls":6},"4号烧结机大修"]
[{"$nulls":6},26]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"齿圈、齿轮","index":6,"n_rows":15,"n_cols":14,"rows_kept":15,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[8,0,8,4],[9,0,9,9],[11,0,11,16],[12,0,12,16],[13,0,13,16],[14,0,14,3],[14,10,14,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":12},"G标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0302010002002","大半齿圈","YH50124-12P改","标件","件",1,{"$nulls":6},"4号烧结机大修"]
[2,"0302010002008","大半齿圈","YH50124-12P",null,"件",1]
[3,"0302010006021","小齿轮装置","YH50128改",null,"套",1,{"$nulls":6},"4号烧结机大修"]
[4,"0302010002018","小齿轮装置","YH50128","制作件","件",1,{"$nulls":6},"4号烧结机大修"]
[{"$nulls":6},4]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"滑板","index":7,"n_rows":14,"n_cols":14,"rows_kept":14,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[7,0,7,4],[8,0,8,9],[10,0,10,16],[11,0,11,16],[12,0,12,16],[13,0,13,3],[13,10,13,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":12},"H标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0302001003001","头滑板","13B400-10-48-1","35SiMn","件",2,{"$nulls":6},"4号烧结机大修"]
[2,"0302001003003","尾滑板","13B400-10-48-3","35SiMn","件",2,{"$nulls":6},"4号烧结机大修"]
[3,"0302001003002","中滑板","13B400-10-48-2","35SiMn","件",136,{"$nulls":6},"4号烧结机大修"]
[{"$nulls":6},140]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]

{"sheet":"阀门","index":8,"n_rows":21,"n_cols":14,"rows_kept":21,"merged":[[0,0,0,2],[1,0,1,14],[2,0,2,3],[14,0,14,4],[15,0,15,9],[17,0,17,16],[18,0,18,16],[19,0,19,16],[20,0,20,3],[20,10,20,13]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-168",{"$nulls":12},"I标段"]
["序号","物料编码","货物名称","规格/型号","技术要求","单位","招标量","单价\n（元）","合计（元）","付款方式","交货期","报价货物品牌/厂家","备注","项目"]
[1,"0510004002197","手动卸灰球阀","DN150 PN1.6MPa  Q41F-16C","带配对法兰、连接件及密封件","台",2,{"$nulls":6},"粗煤气第三批"]
[2,"0510004002198","手动球阀","DN150 PN1.6MPa  Q41F-16C","带配对法兰、连接件及密封件","台",2,{"$nulls":6},"粗煤气第三批"]
[3,"0510004003077","气动卸灰球阀","DN150 PN1.6MPa  Q641F-16C","带配对法兰、连接件及密封件；卸灰球阀，带气动三联件，直流24V双线圈和接近开关，防爆防水防尘防静电；驱动用气连接软管2米长;带配对法兰、连接件及密封件","台",2,{"$nulls":6},"粗煤气第三批"]
[4,"0510004003094","气动球阀","DN150 PN1.6MPa  Q641F-16C","带配对法兰、连接件及密封件；带气动三联件，直流24V双线圈和接近开关，防爆防水防尘防静电；驱动用气连接软管2米长;","台",2,{"$nulls":6},"粗煤气第三批"]
[5,"0510015001023","φ400放散阀","LLSS44Y-2.5  DN400  PN0.25MPa","阀门配带钢丝绳9NAT6X19+FC1770ZZ长度约40m;配带φ250滑轮4个；配带配对法兰、连接件及密封件，阀门卷扬机利旧","个",1,{"$nulls":6},"粗煤气第三批"]
[6,"0510021002102","安全泄压/持压阀","AX742X-10型 DN40 ","开启压力0.78MPa 带配对法兰及连接件","件",1,{"$nulls":6},"粗煤气第三批"]
[7,"0203025021","人孔","Ib-8.8A600-1.0（NM-硅胶垫）","HG/T  21517-2014","个",12,{"$nulls":6},"粗煤气第五批"]
[8,"0203025020","人孔","II（AG）600-0.6  H1=250 DN600","HG/T 21516-2014","台",7,{"$nulls":6},"粗煤气第三批"]
[9,"0510004003093","气动卸灰球阀","Q641F-16C DN300","带配对法兰及连接件及密封件；配带气动三连件，直流24V双线圈电磁阀和接近开关，防爆、防水、防尘、防静电；驱动用气连接软管2m长。","个",4,{"$nulls":6},"粗煤气第五批"]
[10,"0510014001033","调压阀组","φ1800","（现场操作、防爆操作箱。三个DN800的调节阀扭矩大于6100，DN400常调扭矩5100.高压侧压力最高2.5MPa，最高煤气量小时30万）带配套法兰、金属垫及紧固件","套",1,{"$nulls":5},"技术要求详见附件8","热风炉第一批"]
[{"$nulls":6},34]
["投标总价：  佰  拾  万  仟  佰  拾  元整（大写） ",{"$nulls":9},"¥          元"]
["注："]
["    1、单价为含税到厂价，一票结算，税率13%。"]
["    2、报价时请务必注明付款方式。"]
[]
["投标人（章）：",{"$nulls":9},"2021年  月  日于首钢长钢"]