{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["标段1（双金属）","标段2（无缝管及焊管）","标段3（新增）"],"not_rendered":{"external_links":1,"defined_names":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"标段1（双金属）","index":0,"n_rows":18,"n_cols":16,"rows_kept":18,"merged":[[0,0,0,2],[1,0,1,14],[2,3,2,11]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-228",null,null,"项目名称：八高炉渣处理系统改造项目（双金属耐磨复合管、弯头等）",{"$nulls":11},"第1标段"]
["序号","物料编码","货物名称","规格","型号","单位","招标量","单价  \n（元）","合计（元）","付款方式","报价货物品牌/厂家","交货期","修订型号","修订标准","备注","申报单位"]
[1,"0502003001358","双金属耐磨复合管","D426×9  ","组合 执行DL/T680-2015，外无缝管厚9mm,内衬高铬镍合金8mm","米",4,{"$nulls":8},"QG2021091700011676"]
[2,"0502003001359","双金属耐磨复合管","D478×9","组合 执行DL/T680-2015，外无缝管厚9mm,内衬高铬镍合金8mm","米",40,{"$nulls":8},"QG2021091700011676"]
[3,"0502003001360","双金属耐磨复合管","D630×10","组合 执行DL/T680-2015，外无缝管厚10mm,内衬高铬镍合金8mm","米",83,{"$nulls":8},"QG2021091700011676"]
[4,"0515027004152","双金属耐磨弯头","30°  DN600","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",2,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[5,"0515027004153","双金属耐磨弯头","90°  DN400","组合 执行DL/T695-2014，外管厚9mm,内衬高铬镍合金8mm","个",4,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[6,"0515027004154","双金属耐磨弯头","90°  DN450","组合 执行DL/T695-2014，外管厚9mm,内衬高铬镍合金8mm","个",16,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[7,"0515027004155","双金属耐磨弯头","90°  DN600","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",7,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[8,"0515027038012","双金属耐磨同心异径管","DN450/DN300","组合 执行DL/T695-2014，外管厚9mm,内衬高铬镍合金8mm","个",4,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[9,"0515027038013","双金属耐磨偏心异径管","DN600/DN350","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",4,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[10,"0515028004035","双金属耐磨等径三通","DN600","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",1,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[11,"0515028004036","双金属耐磨异径三通","DN600/DN450","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",4,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[12,"0515028004037","双金属耐磨四通","DN600/DN400","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",2,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[13,"0515028006022","双金属耐磨管堵","DN600","组合 执行DL/T695-2014，外管厚10mm,内衬高铬镍合金8mm","个",3,{"$nulls":7},"配合双金属耐磨复合管使用","QG2021091700011676"]
[null,"合计",{"$nulls":4},174]

{"sheet":"标段2（无缝管及焊管）","index":1,"n_rows":19,"n_cols":16,"rows_kept":19,"merged":[[0,0,0,2],[1,0,1,14],[2,3,2,11],[14,0,14,4]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-228",null,null,"项目名称：八高炉渣处理系统改造项目（螺旋焊管无缝管重轨）",{"$nulls":11},"第2标段"]
["序号","物料编码","货物名称","规格","型号","单位","招标量","单价  \n（元）","合计（元）","付款方式","报价货物品牌/厂家","交货期","修订型号","修订标准","备注","申报单位"]
[1,"0502001001004","重轨","43kg","含252套GDGL-2型钢轨连接件和2套SCL-2型钢轨变形缝连接件","吨",8.484,{"$nulls":7},"GB/T2585-2007 按《05G525》图集标准附带252套GDGL-2型钢轨连接件和2套SCL-2型钢轨变形缝连接件","炼铁厂八高炉渣处理系统改造工程QG2021091700011677"]
[2,"0502003001343","无缝钢管","108*12 材质10 ","要求每支管长不低于12米","吨",15,{"$nulls":7},"GB/T8163-2018","炼铁厂八高炉本体大修QG2021091000011630"]
[3,"0502003004006","焊管","DN50",null,"吨",0.667,{"$nulls":7},"GB/T3091-2015  共126米","QG2021091700011676"]
[4,"0502003004038","螺旋焊管","219*6","Q235B","吨",1.829,{"$nulls":7},"GB/T3091-2015  共58米","QG2021091700011676"]
[5,"0502003004054","螺旋焊管","325*8","Q235B","吨",13.259,{"$nulls":7},"GB/T3091-2015  共212米","QG2021091700011676"]
[6,"0502003004069","螺旋焊管","630*10",null,"吨",16.819,{"$nulls":7},"GB/T3091-2015  共110米","QG2021091700011676"]
[7,"0502003004090","螺旋焊管","273*7",null,"吨",3.536,{"$nulls":7},"GB/T3091-2015  共77米","QG2021091700011676"]
[8,"0502003004106","螺旋焊管","377*9",null,"吨",2.532,{"$nulls":7},"GB/T3091-2015  共31米","QG2021091700011676"]
[9,"0502003004702","螺旋焊管","D1020*14","Q235B","吨",6.947,{"$nulls":7},"GB/T3091-2015  共20米","QG2021091700011676"]
[null,"合计",{"$nulls":4},69.07300000000001]
[" 投标总价：佰 拾  万  仟  佰  拾  元整（大写） ",{"$nulls":5},"¥          元"]
[null,"投标人（章）：",{"$nulls":7},"2021年  月  日于首钢长钢（山西长治）"]
[null,"注：1、单价为含税到厂承兑价，一票结算，税率13%；"]
[null,"    2、报价时请务必注明付款方式和所报品牌、包装规格，交货期；"]
[null,"    3、报价时附U盘Excel形式的电子表一份，不得改变表格顺序，不得删除。"]

{"sheet":"标段3（新增）","index":2,"n_rows":53,"n_cols":17,"rows_kept":53,"merged":[[0,0,0,2],[1,0,1,14],[2,3,2,11],[48,0,48,4]],"flags":["formulas_cached_only"]}
["附件3："]
["投 标 货 物 数 量 及 价 目 表"]
["招标编号：长招办2021-228",null,null,"项目名称：八高炉本体大修等项目（钢材）",{"$nulls":11},"第3标段"]
["序号","物料编码","货物名称","规格","型号","单位","招标量","单价  \n（元）","合计（元）","付款方式","报价货物品牌/厂家","交货期","修订型号","修订标准","备注","申报单位"]
[1,"0502001001003","重轨","38kg",null,"吨",6.972,{"$nulls":8},"炼铁厂4号烧结机系统大修","QG2021091400011661"]
[2,"0502002001003","工字钢","14#","Q235B","吨",1.6,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[3,"0502002001006","工字钢","20#a","Q235B","吨",1.76,{"$nulls":7},"63米，执行标准GB/T706-2008","炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[4,"0502002001008","工字钢","22#a","Q235B","吨",1.49,{"$nulls":7},"45米，执行标准GB/T706-2008","炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[5,"0502002001010","工字钢","25#a","Q235B","吨",3.2,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[6,"0502002002003","槽钢","8#",null,"吨",0.12,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011787"]
[7,"0502002002004","槽钢","10#","Q235B","吨",0.25,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011784"]
[8,"0502002002004","槽钢","10#","Q235B","吨",0.5,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011787"]
[9,"0502002002006","槽钢","14#a","Q235B","吨",0.5,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[10,"0502002002008","槽钢","16#a","Q235B","吨",1,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[11,"0502002002016","槽钢","25#a",null,"吨",0.5,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[12,"0502002007001","扁钢","30*4","Q235B","吨",0.503,{"$nulls":8},"炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[13,"0502002007018","扁钢","100*3","Q235B","吨",0.64,{"$nulls":8},"炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[14,"0502002007038","扁钢","80*8",null,"吨",0.945,{"$nulls":7},"80*8  188米  GB/T700-2006","炼铁厂八高炉出铁场除尘系统改造工程","QG2021093000011813"]
[15,"0502002008012","H型钢","150*150*7*10","Q235B","吨",0.5,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[16,"0502002008018","H型钢","588*300*12*20","Q235B","吨",5.44,{"$nulls":8},"炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[17,"0502002008020","H型钢","250*125*6*9","Q235B","吨",0.8,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[18,"0502002008023","H型钢","390*300*10*16","Q235B","吨",2.57,{"$nulls":8},"炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[19,"0502002008061","H型钢","HM148*100*6*9","Q235B","吨",0.6,{"$nulls":7},"执行标准GB/706-2008","炼铁厂八高炉本体大修","QG2021092800011797"]
[20,"0502003001023","不锈钢无缝管","28*3","304","吨",0.15,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011787"]
[21,"0502003001224","不锈钢无缝管","ф34*4","304 GB/T 14976-2012","吨",0.1,{"$nulls":7},"30米","炼铁厂八高炉本体大修","QG2021092700011786"]
[22,"0502003001224","不锈钢无缝管","ф34*4","304 GB/T 14976-2012","吨",0.12,{"$nulls":7},"30米","炼铁厂八高炉本体大修","QG2021092700011784"]
[23,"0502003001224","不锈钢无缝管","ф34*4","304 GB/T 14976-2012","吨",0.6,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011787"]
[24,"0502003001225","不锈钢无缝管","ф42*4","304 GB/T 14976-2012","吨",0.113,{"$nulls":7},"30米","炼铁厂八高炉本体大修","QG2021092700011786"]
[25,"0502003001225","不锈钢无缝管","ф42*4","304 GB/T 14976-2012","吨",0.15,{"$nulls":7},"30米","炼铁厂八高炉本体大修","QG2021092700011784"]
[26,"0502003001228","不锈钢无缝管","ф60*4","304 GB/T 14976-2012","吨",0.5,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011787"]
[27,"0502003001350","钢管","Φ33.5*3.25 ","材质10  执行标准GB8163-87","吨",0.5,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092800011806"]
[28,"0502003001351","钢管","Φ114*7"," 材质10  执行标准GB8163-87","吨",1.8,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092800011806"]
[29,"0502003001352","钢管","Φ27*3.5"," 材质10  执行标准GB8163-87","吨",0.5,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092800011806"]
[30,"0502003001353","钢管 ","Φ48*3.5"," 材质10  执行标准GB8163-87","吨",0.5,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092800011806"]
[31,"0502003001354","不锈钢无缝管","Φ30*4","不锈钢304","吨",2.5,{"$nulls":7},"304不锈钢","炼铁厂八高炉本体大修","QG2021092700011787"]
[32,"0502003001361","不锈钢无缝管","42*6  304",null,"吨",0.5,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011787"]
[33,"0502003001362","不锈钢无缝管","Φ28*3.5   ","304","吨",1.3,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092700011784"]
[34,"0502003004003","焊管","DN25",null,"吨",0.2,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092800011806"]
[35,"0502003004005","焊管","DN40",null,"吨",0.5,{"$nulls":7},"Q235 GB/T8162-2008","炼铁厂八高炉本体大修","QG2021092800011806"]
[36,"0502003004005","焊管","DN40",null,"吨",1.82,{"$nulls":7},"474米，执行标准GB/T13793-2016","炼铁厂8高炉粗煤气系统大修","QG2021092800011796"]
[37,"0502003004006","焊管","DN50",null,"吨",0.2,{"$nulls":8},"炼铁厂八高炉本体大修","QG2021092800011806"]
[38,"0502003004008","焊管","DN80",null,"吨",0.5,{"$nulls":7},"Q235 GB/T8162-2008","炼铁厂八高炉本体大修","QG2021092800011806"]
[39,"0502004001029","开平板","6mm","Q235B","吨",2,{"$nulls":7},"执行标准GB/T3274-2018","炼铁厂八高炉本体大修","QG2021092800011797"]
[40,"0502004002001","中板","8mm","Q235B","吨",165.353,{"$nulls":7},"2633m2，板宽2.2m","炼铁厂八高炉出铁场除尘系统改造工程","QG2021093000011813"]
[41,"0502004002002","中板","10mm","Q235B","吨",12,{"$nulls":7},"执行标准GB/T3274-2018","炼铁厂八高炉本体大修","QG2021092800011797"]
[42,"0502004003012","花纹钢板","δ=10","Q235B","吨",4,{"$nulls":7},"执行标准GB/T3274-2018","炼铁厂八高炉本体大修","QG2021092800011797"]
[43,"0502004008001","压板","43Kg",null,"块",50,{"$nulls":8},"炼铁厂4号烧结机系统大修","QG2021091400011661"]
[null,"合计",{"$nulls":4},275.79600000000005]
[" 投标总价：佰 拾  万  仟  佰  拾  元整（大写） ",{"$nulls":5},"¥          元"]
[null,"投标人（章）：",{"$nulls":7},"2021年  月  日于首钢长钢（山西长治）"]
[null,"注：1、单价为含税到厂承兑价，一票结算，税率13%；"]
[null,"    2、报价时请务必注明付款方式和所报品牌、包装规格，交货期；"]
[null,"    3、报价时附U盘Excel形式的电子表一份，不得改变表格顺序，不得删除。"]